Run install.bat or follow the manual installation instructions below.

Manual installation instructions
--------------------------------
1. Copy the EAPCI folder to your c:\ drive
2. Copy the provided autoexec.bat file to your c:\ drive or edit your current one.
3. Copy the provided config.sys file to your c:\ drive or edit your current one.
4. If you have any problems getting your setup to work make sure your card is supported and view the important notes below.



The ENSONIQ.zip archive contains the dos sound card drivers for creative labs ensoniq audio pci cards. They are setup and optimized for ArcadeOS and MAME but they should work well with any legacy dos game.

ENSONIQ.zip supports the following Creative Labs PCI sound cards
-------------------------------------------------------------
Sound Blaster AudioPCI
Ensoniq AudioPCI
Any of the following chipsets: 1370, 1371, 1373



Important Notes:

1. Your sound blaster pci card can not use irq 5.
2. Your sound blaster pci card should not use the same irq as your video card.
3. You must first uninstall your current sound blaster dos drivers in Windows for the ENSONIQ drivers to work (Start/Settings/Control Panel/Add Remove Programs/Your Sound Card).